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 Safe Solution( Econo Pack application instructions

IDEAL FOR SMALLER JOBS SUCH AS:

Entranceways * Hot Tub Surrounds * Steps * Patios * Kitchens & more!

Each Econo Pack Safe Solution( Kit covers approximately 40 square metres
USE ONLY AS DIRECTED

TO APPLY TREATMENT (use under well ventilated conditions)

For use on Porcelain/Steel Enamel Bathtubs, follow instructions on bottles.

For use on Ceramic Tile, Quarry Tile and Granite Surfaces, follow instructions below.

BEFORE YOU START YOU WILL NEED: Rubber sole boots, protective gloves (included), one 20 L wringer pail, two string mops, a mask for you face (included, if you have a poor ventilated area), safety goggle (included), plastic sheet to place the chemicals, rug to assist drying surface.

Step 1

Be sure to remove all movable objects off the areas to be treated.  Fill wringer pail ½ full with hot water and add the bottle of Prep/Cleaner Solution.

Step 2

Begin mopping out the Prep/Cleaner Solution, using one of the string mops.  Do not splash against walls or appliances.  When coming up to carpets or door thresholds, give yourself approximately one or two inches from the edge. 

Step 3

Remove the Prep/Cleaner Solution using wringer pail, mop and hot water.  Be sure the Prep/Cleaner is completely rinsed off the surface to be treated.  Allow surface to dry.

Step 4

Fill wringer pail ½ full with hot water and add bottle of neutralizer Solution, then set pail aside (you will need it for the final step).  Using the other new string mop, pour the Safe Solution( Treatment onto the mop and begin mopping carefully.  Do not Splash against walls or appliances.  When coming up to carpets or door thresholds give yourself approximately one or two inches.  Be sure to get entire area wet with Safe Solution( Treatment.  Do not allow any areas to dry during this procedure.  Leave treatment down for approximately 5 to 10 minutes until you feel that there is a good traction under your feet. Please note some tiles might require longer time to be treated.

Note: During the Safe Solution application, do not move off area until your feet and the area is neutralized using the Neutralizer Solution, otherwise you will carry the acid on your feet and mark other area or damage other surface.
Step 5

Place the mop that you have been using to treat the surface into the pail that you set aside in Step 4 and begin to mop out the Neutralizer Solution over entire treated surface, being careful not to splash.  Now clean up with hot water.  Your treated surface is now ready to use.

CAUTION: 

Although Safe Solution( greatly increases traction – please continue to use caution on the areas treated.  

Not for use on marble, vinyl, wood, cement, or acrylic surfaces.

Keep out of reach of children.

Always wear protective gloves while using the chemicals and goggle when there is any chance to splash into eye. 

If Safe Solution© is accidentally spilled onto skin, wash off immediately using running water. For detailed instructions refer to Safe Solution MSDS sheet Section 4, First Aid measures and seek medical attention.  

For all chemicals, refer to enclosed MSDS sheets.

Questions? Toll free: 1300 668 620 (24 hours / 365 days)
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