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-FLOOR SAFETY INSPECTION REPORT-





~ SLIP RESISTANCE CONDITION OF SURFACE ~

1. Initial slip-resistance test (Use water only):

(√ Check appropriate box)

 FORMCHECKBOX 
 Excellent

 FORMCHECKBOX 
 Fair

 FORMCHECKBOX 
 Poor
2. Final slip-resistance test (Use Maintenance Solution™ diluted 1:10):

(√ Check appropriate box)

 FORMCHECKBOX 
 Excellent

 FORMCHECKBOX 
 Fair

 FORMCHECKBOX 
 Poor

(√ Check appropriate box)

Did slip-resistance recover when cleaned with Maintenance Solution™?  FORMCHECKBOX 
 Yes
 FORMCHECKBOX 
 No
(If No then floor requires rejuvenating)

EQUIPMENT CHECK:

(√ Check appropriate box if okay) 
 FORMCHECKBOX 
 Mop buckets 
 FORMCHECKBOX 
 Mops  
 FORMCHECKBOX 
 Deck brush
If not okay please explain:

(Dirty mops, Dirty mop buckets, Worn Brush, etc.)

CLEANERS CHECK (If not using Maintenance Solution™)
(√ Check appropriate box)

 FORMCHECKBOX 
 Acceptable

 FORMCHECKBOX 
 Unacceptable

If unacceptable please explain:

(Powders, Abrasives, Bleach, etc.)

Is a training session with cleaning staff recommended? (√ Check appropriate box)   FORMCHECKBOX 
 Yes
 FORMCHECKBOX 
 No

If Yes, please arrange appropriate time: 
Day/ 

Month/ 
Year/


DOES FLOOR REQUIRE REJUVENATING? (√ Check appropriate box)   FORMCHECKBOX 
 Yes

 FORMCHECKBOX 
 No
If Yes, please arrange appropriate time: 
Day/ 

Month/ 
Year/

Detailed report:

Area surface is tiled using 2 different tiles. Surface generally quite dirty and also has other contaminants on the floor like chewing gums, patches. Tested slip resistive qualities on ground floor and found to be unacceptable slippery, especially that ground floor level entrance frequently flooded from outside. There is also a potential slip and trip hazard due to badly broken tile on first stair.  

Floor pictures below. 
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Tiled entrance that gets flooded  Broken tile slip trip hazard       Badly broken tile slip trip hazard 
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Area treated with Safe Solution(. Excellent slip resistive quality. Picture taken using flash.

Recommendations:

As the area surface slip natural resistive features are very low, it is recommended to treat the area with Safe Solution( Anti-slip treatment, then follow-up with regular cleaning regime preferably monthly, but at least quarterly.  Replace broken tiles on stairs, especially at entrance as it is very hazardous.

Inspector:  Tibor Bode
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E-mail:








City: Cabramatta








Job Address: 146 Barry street
























































Customer Name: XYZ Pty Ltd








Contact Name: Mr John Smith








Date: 17/9/2004






































State: NSW








Telephone: 9455 9999








Facsimile: 3222 3412








Inspected By: Tibor Bode








Total Area Size: 32.5sqm








Area Inspected: Stairs and entrance areas























